SECUMAX · Destination Security
Recorder Quick Start Guide

1. Before you start
Check the package contents against the packing list and confirm the power supply matches the specification on the product label.
2. Mounting
Mark the mounting holes using the supplied template. Use the included anchors for concrete or brick, and seal cable entries for outdoor installations.
3. Wiring & power
Connect power and data as shown in the product datasheet. For PoE devices use a Cat5e/Cat6 cable up to 100 m.
4. Configuration
Power on the device and complete setup through the recorder, controller or mobile app. Change the default password on first login.
5. Support
Need help? Contact Secumax technical support: sales@secumax.org | +971 4 123 4567.
